Jan 12, 2019 19:57:08.782 [0x7f696d7ff700] INFO - Plex DLNA Server v1.14.1.5488-cc260c476 - ubuntu PC x86_64 - build: linux-ubuntu-x86_64 - GMT 13:00
Jan 12, 2019 19:57:08.784 [0x7f696d7ff700] INFO - Linux version: 4.9.0-8-amd64 (#1 SMP Debian 4.9.130-2 (2018-10-27)), language: en-NZ
Jan 12, 2019 19:57:08.784 [0x7f696d7ff700] INFO - Processor Intel(R) Core(TM) i5 CPU       M 480  @ 2.67GHz
Jan 12, 2019 19:57:08.789 [0x7f69752147c0] DEBUG - Unique device name = 283164fc-0a35-82db-04b6-39ef001ace07
Jan 12, 2019 19:57:08.789 [0x7f69752147c0] DEBUG - DLNA server port: 32469
Jan 12, 2019 19:57:08.789 [0x7f69752147c0] DEBUG - PMS: http://127.0.0.1:32400/
Jan 12, 2019 19:57:08.789 [0x7f69752147c0] DEBUG - MyPlex: https://plex.tv/
Jan 12, 2019 19:57:20.777 [0x7f69752147c0] DEBUG - Reading system DLNA client profiles
Jan 12, 2019 19:57:21.644 [0x7f69752147c0] DEBUG - Reading user client profile "50DX700"
Jan 12, 2019 19:57:21.679 [0x7f69752147c0] DEBUG - Reading user client profile "50CX700"
Jan 12, 2019 19:57:21.717 [0x7f69752147c0] DEBUG - Read 24 DLNA client profiles
Jan 12, 2019 19:57:21.732 [0x7f69752147c0] DEBUG - [PERF] Slowest insertShortKey in 10.000000 ms.
Jan 12, 2019 19:57:21.741 [0x7f69752147c0] DEBUG - DLNA device discovery enabled every 60 seconds
Jan 12, 2019 19:57:21.791 [0x7f69752147c0] DEBUG - Initialization complete
Jan 12, 2019 19:57:22.157 [0x7f6957fff700] DEBUG - OnGetProtocolInfo from 192.168.1.5
Jan 12, 2019 19:57:22.158 [0x7f6957fff700] DEBUG - Mapped client to generic profile: X-AV-Physical-Unit-Info: pa="UBP-X800";; X-AV-Client-Info: av=5.0; cn="Sony Corporation"; mn="UBP-X800"; mv="2.0";; Host: 192.168.1.200:32469; User-Agent: UPnP/1.0 DLNADOC/1.50; Content-Length: 273; Content-Type: text/xml; charset="utf-8"; SOAPACTION: "urn:schemas-upnp-org:service:ConnectionManager:1#GetProtocolInfo"
Jan 12, 2019 19:57:22.404 [0x7f6956ffd700] DEBUG - Device 50CX700_Series at 192.168.1.6 will use Panasonic VIErA TH-50CX700Z TV profile
Jan 12, 2019 19:57:22.405 [0x7f6958fff700] DEBUG - Device 50CX700_Series at 192.168.1.6 will use Panasonic VIErA TH-50CX700Z TV profile
Jan 12, 2019 19:57:22.411 [0x7f6963bff700] DEBUG - Device 50CX700_Series at 192.168.1.6 will use Panasonic VIErA TH-50CX700Z TV profile
Jan 12, 2019 19:57:22.456 [0x7f69547f8700] DEBUG - OnGetProtocolInfo from 192.168.1.5
Jan 12, 2019 19:57:22.456 [0x7f69547f8700] DEBUG - Mapped client to generic profile: X-AV-Physical-Unit-Info: pa="UBP-X800";; X-AV-Client-Info: av=5.0; cn="Sony Corporation"; mn="UBP-X800"; mv="2.0";; Host: 192.168.1.200:32469; User-Agent: UPnP/1.0 DLNADOC/1.50; Content-Length: 273; Content-Type: text/xml; charset="utf-8"; SOAPACTION: "urn:schemas-upnp-org:service:ConnectionManager:1#GetProtocolInfo"
